{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","SEHVX-AAW"]
[]
[]
[]
[]
["","","","","SEHVX20AAW","SEHVX32AAW","SEHVX40AAW","SEHVX64AAW"]
["Chladivo","Vliv na globální oteplování (GWP)","","","","2,087.5"]
["","Typ","","","","R-410A"]
["Rozměry","Jednotka","Šířka","mm","","766"]
["","","Hloubka","mm","","396"]
["","","Výška","mm","","1,573"]
["Opláštění","Materiál","","","","Polyesterem lakovaný pozinkovaný ocelový plech"]
["","Barva","","","","Bílá Daikin"]
["Hmotnost","Jednotka","","kg","","62"]
["Power supply","Fáze","","","","3N~"]
["","Frekvence","","Hz","","50"]
["","Označení","","","","W1"]
["","Napětí","","V","","400"]
["Poznámky","","","","(1) - Včetně potrubí + PHE; bez expanzní nádoby","(1) - Včetně potrubí + PHE; bez expanzní nádoby","(1) - Včetně potrubí + PHE; bez expanzní nádoby","(1) - Včetně potrubí + PHE; bez expanzní nádoby"]
["","","","","(2) - Bez vody v jednotce. Minimální objem vody je dostatečný pro většinu aplikací. Při velkém namáhání může být potřeba více vody.","(2) - Bez vody v jednotce. Minimální objem vody je dostatečný pro většinu aplikací. Při velkém namáhání může být potřeba více vody.","(2) - Bez vody v jednotce. Minimální objem vody je dostatečný pro většinu aplikací. Při velkém namáhání může být potřeba více vody.","(2) - Bez vody v jednotce. Minimální objem vody je dostatečný pro většinu aplikací. Při velkém namáhání může být potřeba více vody."]
["","","","","(3) - Bez objemu vody v jednotce. Tento objem zaručí dostatečnou odmrazovací energii pro všechny aplikace, avšak lze jej vynásobit 0,66, pokud je bod nastavení vytápění ≥ 45° C (např. fan-coily)","(3) - Bez objemu vody v jednotce. Tento objem zaručí dostatečnou odmrazovací energii pro všechny aplikace, avšak lze jej vynásobit 0,66, pokud je bod nastavení vytápění ≥ 45° C (např. fan-coily)","(3) - Bez objemu vody v jednotce. Tento objem zaručí dostatečnou odmrazovací energii pro všechny aplikace, avšak lze jej vynásobit 0,66, pokud je bod nastavení vytápění ≥ 45° C (např. fan-coily)","(3) - Bez objemu vody v jednotce. Tento objem zaručí dostatečnou odmrazovací energii pro všechny aplikace, avšak lze jej vynásobit 0,66, pokud je bod nastavení vytápění ≥ 45° C (např. fan-coily)"]
["","","","","","(4) - Zařízení využívá fluorované skleníkové plyny"]
["Opláštění","Barva","","","Bílá Daikin","","Bílá Daikin","Bílá Daikin"]
["","Materiál","","","Polyesterem lakovaný pozinkovaný ocelový plech","","Polyesterem lakovaný pozinkovaný ocelový plech","Polyesterem lakovaný pozinkovaný ocelový plech"]
["Rozměry","Jednotka","Výška","mm","1573","","1573","1573"]
["","","Šířka","mm","766","","766","766"]
["","","Hloubka","mm","396","","396","396"]
["Hmotnost","Jednotka","","kg","60","","64","66"]
["Chladivo","Typ","","","R-410A","","R-410A","R-410A"]
["","Vliv na globální oteplování (GWP)","","","2087.5","","2087.5","2087.5"]
["Napájení","Označení","","","W1","","W1","W1"]
["","Fáze","","","3N~","","3N~","3N~"]
["","Frekvence","","Hz","50","","50","50"]
["","Napětí","","V","400","","400","400"]