{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKCBH-BBV3"]
[]
[]
[]
[]
["","","","","EKCBH008BBV3"]
["Rozměry","Jednotka","Šířka","mm","412"]
["","","Hloubka - s dálkov ým ovládáním montovan é na přední desce","mm","120"]
["","","Hloubka","mm","100"]
["","","Výška","mm","390"]
["Hmotnost","Jednotka","","kg","6"]
["Pomocný ohřívač","Napájení","Fáze","","1~, 3~"]
["","","Napětí","V","230, 400"]
["","","Frekvence","Hz","50"]
["Poznámky","","","","(1) - Ovennævnte strømforsyning til hydroboksen er kun til sikkerhedsvarmeren. Kontaktboksen og pumpe for hydroboks forsynes via den udendørs enhed. Boligens valgfrie varmtvandsbeholder har separat strømforsyning."]
["","","","","(2) - V závislosti na nastavení priority záložního ohřívače mohou nebo nemohou souprava záložního ohřívače EKMBUH* a pomocného ohřívače fungovat souběžně."]
["","","","","(3) - Podrobnosti viz instalační příručka EBHQ*; specifikace soupravy záložního ohřívače viz specifikace EKMBUH*"]
["","","","","(4) - Kabelové spoje: zvolte průměr a typ podle státních a místních předpisů; Podrobnosti k rozsahům napětí a proudů viz instalační příručka EBHQ*"]
["","","","","(5) - Napájení se vztahuje ke kombinaci s EKHW*V3 příp. EKHW*Z2."]