{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Hladina akustického tlaku","Vytápění","Vysoké","dBA","38"]
["","","Střední","dBA","36"]
["","","Nízký","dBA","30"]
["","Chlazení","Střední","dBA","36"]
["","","Nízký","dBA","30"]
["","","Vysoké","dBA","38"]
["Standardní příslušenství","Příručka pro instalaci","","","1"]
["","Manuální ovládání","","","1"]
["","Izolace pro upevnění","","","1"]
["","Těsnicí podložky","","","1"]
["","Kovová svorka","","","1"]
["","Drenážní hadice","","","1"]
["","Podložka pro konzoli závěsu","","","8"]
["","Těsnící materiál","","","2"]
["","Svorky","","","6"]
["","Upínací deska podložky","","","4"]
["","Šrouby pro příruby kanálu","","","1"]
["","Vzduchový filtr","","","1"]
["Spoje potrubí","Kapalina","Vnější průměr","mm","6.35"]
["","Plyn","Vnější průměr","mm","12.7"]
["","Vypouštění","","","VP20 (I.D. 20/O.D. 26)"]
["Vstup napájení","Chlazení","Jm.","kW","0.060"]
["","Vytápění","Jm.","kW","0.060"]
["Hladina akustického výkonu","Chlazení","","dBA","55"]
["","Vytápění","","dBA","55"]
["Rozměry","Jednotka","Šířka","mm","1,150"]
["","","Hloubka","mm","620"]
["","","Výška","mm","200"]
["Hmotnost","Jednotka","","kg","30.0"]
["Ventilátor","Vnější statický tlak","Jmen.","Pa","40"]
["Power supply","Fáze","","","1~"]
["","Frekvence","","Hz","50/60"]
["","Označení","","","VE"]
["","Napětí","","V","220-240"]
["Poznámky","","","","(1) - Læs specifikationer til den Multi udendørs enhed, der skal tilsluttes, når den er koblet til udendørs enhed i Multi-system."]